PHASE 1: Problem Definition and Design Thinking

# PROJECT: TRAFFIC MANAGEMENT SYSTEM

**Problem Definition:**

Urban areas face significant traffic congestion, leading to increased travel times, safety hazards, environmental pollution, and overall inefficiency. Existing traffic management systems often lack adaptability and integration of real-time data sources. Thus, there is a critical need to develop an IoT-based Traffic Management System that can effectively address these challenges by optimizing traffic flow, enhancing safety, reducing environmental impact, and improving overall urban mobility.

The problem at hand is the inefficient management of urban traffic, resulting in congestion, increased travel times, safety concerns, and environmental issues. This project aims to address this problem by developing an intelligent Traffic Management System (TMS) using IoT technologies. The key issues to be resolved include:

1. **Congestion and Delays:** Urban areas often experience traffic congestion during peak hours, leading to extended travel times and driver frustration.
2. **Safety Concerns:** Inefficient traffic management can contribute to accidents and collisions, endangering the lives of motorists and pedestrians.
3. **Environmental Impact:** Prolonged idling and stop-and-go traffic contribute to increased emissions, air pollution, and fuel consumption, negatively impacting the environment.
4. **Lack of Adaptive Control:** Existing traffic signal systems often operate on fixed schedules, leading to suboptimal traffic flow and inefficient resource utilization.
5. **Data Fragmentation:** There is a wealth of traffic-related data available from various sources, such as sensors, cameras, and GPS devices, but it is often underutilized or not integrated effectively.
6. **Ineffective Routing:** Traditional navigation systems do not adapt to real- time traffic conditions, leading to suboptimal routing decisions.
7. **Predictive Insights:** There is a need for predictive analytics to anticipate traffic patterns, accidents, and congestion events, allowing for proactive management.
8. **Communication and Coordination:** Effective communication and coordination between traffic signals, sensors, and vehicles are essential for a responsive traffic management system.
9. **User Experience:** The system should consider the user experience for both drivers and pedestrians by providing real-time updates and alternate routes.

The goal of this project is to develop a comprehensive IoT-based Traffic Management System that addresses these issues by seamlessly integrating data from various sources, implementing adaptive signal control, optimizing routing, and providing predictive insights to enhance traffic flow, safety, and environmental sustainability in urban areas.

# Design Thinking:

Design thinking for an IoT-based Traffic Management System involves several key steps, including defining objectives, sensor design, and various other considerations. Here's a structured approach:

## Objective Definition:

**Understand the Problem:** Begin by gaining a comprehensive understanding of the traffic management challenges in the chosen urban area. Identify key objectives such as reducing congestion, enhancing safety, and minimizing environmental impact.

**Set Clear Objectives:** Define specific, measurable, and achievable objectives for the IoT-based Traffic Management System. For example:

Reduce peak-hour congestion by 30%. Decrease the number of accidents by 20%. Lower carbon emissions by 15%.

## Empathize:

**User Needs Analysis:** Conduct surveys, interviews, and observations to understand the needs and pain points of commuters, pedestrians, traffic authorities, and city planners.

## Define:

**Problem Definition:** Clearly define the problem you aim to solve. For instance, "Develop an IoT-based Traffic Management System to optimize traffic flow, enhance road safety, and reduce environmental impact in urban areas."

## Ideate:

**Brainstorm Solutions:** Organize brainstorming sessions with your team to generate ideas for the system. Consider technologies, approaches, and features that could address the defined problem.

## Prototype:

**Sensor Design:** Develop sensor prototypes or specifications tailored to your system's objectives:

**Traffic Flow Sensors:** Design sensors that can detect vehicle presence, count, and speed to monitor traffic flow.

**Safety Sensors:** Create sensors capable of identifying safety hazards, such as sudden stops or erratic driving behaviour.

**Environmental Sensors**: Develop sensors to measure air quality and emissions.

**Communication Sensors:** Include communication modules to facilitate data transmission.

## Test:

**Sensor Testing:** Evaluate the performance of the sensor prototypes in a controlled environment to ensure they meet accuracy and reliability requirements.

## Iterate:

**Refine Sensors**: Based on the test results, iterate on the sensor design to improve accuracy, durability, and efficiency.

## Implement:

**Full System Development:** Combine the refined sensors with the IoT platform and software components to create the complete Traffic Management System.

## Monitor and Gather Data:

**Deployment:** Install the sensors and the system infrastructure in the selected urban area.

**Data Collection:** Continuously gather real-time data from the deployed sensors, including traffic flow, safety incidents, and environmental metrics.

## Feedback Loop:

**Data Analysis:** Analyse the collected data to identify traffic patterns, congestion hotspots, safety issues, and environmental impact.

**User Feedback:** Engage with users and stakeholders to gather feedback on the system's effectiveness and user experience.

## Iterate:

**System Enhancement:** Based on data analysis and user feedback, iterate on the system's algorithms and functionalities to further optimize traffic management.

## Scale and Expand:

**Scaling:** Consider expanding the system to cover more areas or cities as its effectiveness is demonstrated.

**Partnerships:** Explore partnerships with local government agencies and transportation companies to support the system's growth.

Team members:

1. KAVIYA T V 2021504016

2. ANUSNEKHAA L N 2021504503

3. DAINTY CHRISTIANA J C R 2021504509

4. HARITHRA R 2021504520

**PHASE 2:INNOVATION**

After thorough research and analysis, we arrived at an innovative solution to solve the above problem as detailed in phase 1 of our project.

* We will be using Raspberry Pi for the project. It is chosen for smart traffic management due to its affordability, compact size, low power consumption, GPIO pins for sensor integration, connectivity options, customizability with various operating systems, extensive software support, reliability, scalability, and open-source nature, making it a cost-effective and versatile solution for tasks like traffic monitoring, data collection, and signal control in traffic management systems.

**SENSORS:**

* **Camera Module:** The Raspberry Pi Camera captures real-time images and video footage of traffic flow. These visuals provide valuable insights into traffic conditions, allowing for real-time analysis.
* **Ultrasonic Sensors:** Ultrasonic sensors detect the presence of vehicles and measure the distance between vehicles. This data is crucial for understanding traffic density and congestion levels.
* **IR Sensors:** Infrared sensors are used for proximity detection and object recognition. They help in identifying obstacles or vehicles approaching specific areas, enabling efficient traffic management.

**CONNECTIVITY:**

**Wi-Fi Dongle:** If wired Ethernet connection is not feasible, a Wi-Fi dongle provides wireless connectivity, enabling Raspberry Pi to connect to the internet and transmit data to Azure cloud services.

**AZURE CLOUD COMPONENTS:**

**Azure IoT Hub**: Azure IoT Hub serves as the bridge between the Raspberry Pi-based system and the cloud. It enables secure communication, monitoring, and management of IoT devices, ensuring seamless data transmission.

**Azure Blob Storage:** Images and video footage captured by the Raspberry Pi Camera are stored in Azure Blob Storage. Storing this visual data in the cloud allows for historical analysis, pattern recognition, and evidence retrieval if needed.

**Azure Stream Analytics:** Stream Analytics processes real-time data streams from sensors and cameras. It performs instant data analysis, detecting traffic patterns, congestion points, and unusual events, facilitating timely responses.

**Azure Functions:** Azure Functions, based on serverless computing, are triggered by IoT data. They execute specific tasks in response to predefined events, enhancing automation and enabling customized actions based on real-time traffic conditions.

**Azure Web Apps:** Azure Web Apps create user-friendly dashboards and interfaces. These interfaces visualize traffic data, providing real-time updates to traffic authorities and the public. Users can access traffic information easily through web browsers or mobile devices.

**Azure Cosmos DB (or other Database service):** Azure Cosmos DB, a NoSQL database service, stores structured data from sensors and traffic events. It facilitates historical analysis, allowing traffic authorities to identify long-term trends, plan infrastructure changes, and optimize traffic management strategies.

**Azure Virtual Machines (optional):** Azure Virtual Machines can host custom applications or services related to traffic management. These applications can perform complex computations, machine learning algorithms, or AI-driven analytics to enhance traffic prediction and optimize traffic flow further.

**PROTOCOL**

**HTTP:**HTTP is an excellent choice for web based traffic management applications that require user interfaces and real time information delivery to end-users. They are suitable for traffic-related websites, mobile apps and dashboards.

**PUBLIC PLATFORM**

We are going to create a web-based or mobile dashboard to visualize real-time traffic data and system status.

Team members:

1. KAVIYA T V 2021504016

2. ANUSNEKHAA L N 2021504503

3. DAINTY CHRISTIANA J C R 2021504509

4. HARITHRA R 2021504520

**PHASE 3:**

**PROBLEM:**

To develop the python script on IoT devices as per the project requirement.

**SOLUTION:**

The Python script for IoT devices in the project utilizes the ‘machine’ and ‘utime’ module to control traffic lights based on received ultrasonic sensor commands, facilitating traffic management and signal changes.

**SOURCE CODE:**

import machine

import utime

# GPIO pins for the HC-SR04 sensor

trigger\_pin = machine.Pin(2, machine.Pin.OUT)  # Connect to the sensor's trigger pin

echo\_pin = machine.Pin(3, machine.Pin.IN)      # Connect to the sensor's echo pin

# Traffic light control pins (simulated)

red\_light = machine.Pin(10, machine.Pin.OUT)

yellow\_light = machine.Pin(11, machine.Pin.OUT)

green\_light = machine.Pin(12, machine.Pin.OUT)

# Function to measure distance using the HC-SR04 sensor

def measure\_distance():

    trigger\_pin.value(0)

    utime.sleep\_us(2)

    trigger\_pin.value(1)

    utime.sleep\_us(10)

    trigger\_pin.value(0)

    while echo\_pin.value() == 0:

        pulse\_start = utime.ticks\_us()

    while echo\_pin.value() == 1:

        pulse\_end = utime.ticks\_us()

    pulse\_duration = utime.ticks\_diff(pulse\_end, pulse\_start)

    distance = (pulse\_duration \* 0.0343) / 2  # Speed of sound is approximately 343 meters per second

    return distance

# Traffic light control function

def control\_traffic\_lights(distance):

    if distance < 10:  # If a vehicle is very close

        red\_light.value(0)

        yellow\_light.value(1)

        green\_light.value(0)

    elif 10 <= distance < 20:  # If a vehicle is moderately close

        red\_light.value(1)

        yellow\_light.value(0)

        green\_light.value(0)

    else:  # If no vehicle is detected

        red\_light.value(0)

        yellow\_light.value(0)

        green\_light.value(1)

while True:

    distance = measure\_distance()

    # Control traffic lights based on the distance measurements

    control\_traffic\_lights(distance)

    # For simulation purposes, print the distance and the traffic light state


    print("Distance: {:.2f} cm".format(distance))


    utime.sleep(2)  # Wait for a few seconds before taking the next measurement


**LINK:**

[**https://wokwi.com/projects/378915192728578049**](https://wokwi.com/projects/378915192728578049)

**SIMULATION:**

****

****

****

Team members:

1. KAVIYA T V 2021504016

2. ANUSNEKHAA L N 2021504503

3. DAINTY CHRISTIANA J C R 2021504509

4. HARITHRA R 2021504520

**PHASE 4:**

**In this technology project you will continue building your project by developing the platform as per project requirement. Use web development technologies wherever needed. After performing the relevant activities create a document around it and share the same for assessment.**

**ABOUT AZURE:**

Azure is Microsoft's cloud computing platform offering a broad range of cloud services, including infrastructure, platforms, and software. It enables businesses to build, deploy, and manage applications and services in Microsoft-managed data centers. Azure supports virtual machines, databases, AI, IoT, and more, with global data center coverage, robust security, and a pay-as-you-go pricing model. Its scalability, developer tools, and integration with Microsoft services make it a popular choice for organizations seeking cloud solutions to drive innovation, streamline operations, and meet their digital transformation needs.

**Code to display Real time Transit Information azure:**

pip install requests

import requests

import azure.functions as func

def main(req: func.HttpRequest) -> func.HttpResponse:

# Replace with your actual transit API endpoint

api\_endpoint = "https://your-transit-api.com/realtime"

# Replace with your API credentials if needed

api\_headers = {"Authorization": "Bearer YOUR\_API\_KEY"}

response = requests.get(api\_endpoint, headers=api\_headers)

if response.status\_code == 200:

transit\_data = response.json()

return func.HttpResponse(transit\_data, mimetype="application/json")

else:

return func.HttpResponse("Failed to retrieve transit data", status\_code=500)

**Code for Interfacing Data with Azure:**

import machine

import utime

from azure.iot.device import IoTHubDeviceClient, Message

# Define Azure IoT Hub connection string and device ID

CONNECTION\_STRING = "HostName=TrafficManagement.azure-devices.net;DeviceId=RaspPi;SharedAccessKey=7ryCImqSUWqhp5ChKRrkZxNCwpjqtJHL2AIoTGkwJBs="

DEVICE\_ID = "RaspPi"

# Initialize the IoT Hub client

client = IoTHubDeviceClient.create\_from\_connection\_string(CONNECTION\_STRING)

# GPIO pins for the HC-SR04 sensor

trigger\_pin = machine.Pin(2, machine.Pin.OUT)

echo\_pin = machine.Pin(3, machine.Pin.IN)

# Traffic light control pins (simulated)

red\_light = machine.Pin(10, machine.Pin.OUT)

yellow\_light = machine.Pin(11, machine.Pin.OUT)

green\_light = machine.Pin(12, machine.Pin.OUT)

def measure\_distance():

trigger\_pin.value(0)

    utime.sleep\_us(2)

    trigger\_pin.value(1)

    utime.sleep\_us(10)

    trigger\_pin.value(0)

    while echo\_pin.value() == 0:

        pulse\_start = utime.ticks\_us()

    while echo\_pin.value() == 1:

        pulse\_end = utime.ticks\_us()

    pulse\_duration = utime.ticks\_diff(pulse\_end, pulse\_start)

    distance = (pulse\_duration \* 0.0343) / 2  # Speed of sound is approximately 343 meters per second

    return distance

def control\_traffic\_lights(distance):

if distance < 10:

red\_light.value(0)

yellow\_light.value(1)

green\_light.value(0)

elif 10 <= distance < 20:

red\_light.value(1)

yellow\_light.value(0)

green\_light.value(0)

else:

red\_light.value(0)

yellow\_light.value(0)

green\_light.value(1)

while True:

distance = measure\_distance()

control\_traffic\_lights(distance)

# For simulation purposes, print the distance and the traffic light state

print("Distance: {:.2f} cm".format(distance))

# Send distance data to IoT Hub

telemetry\_data = {"distance\_cm": distance}


message = Message(telemetry\_data)

client.send\_message(message)


utime.sleep(2) # Adjust the sleep duration as needed

**Steps we followed while working with Azure:**

1. We created an IoT Hub in Microsoft Azure and Deployed it.



1. We created a Device Id, RaspPi and created a Primary Connection String, by using this, we interfaced it with our Wowki Code, to establish the web application:



**DeviceID:** RaspPi

**Primary Connection string**: HostName=TrafficManagement.azure-devices.net;DeviceId=RaspPi;SharedAccessKey=7ryCImqSUWqhp5ChKRrkZxNCwpjqtJHL2AIoTGkwJBs=

The remaining step is to integrate this code in wokwi, importing azure.iot.device which is already installed using the command**:**

**pip intall azure-iot-devices**

Team members:

1. KAVIYA T V 2021504016

2. ANUSNEKHAA L N 2021504503

3. DAINTY CHRISTIANA J C R 2021504509

4. HARITHRA R 2021504520

**PHASE 5**:

**OBJECTIVE**:

The objective of a traffic management project is to improve the efficiency, safety, and flow of traffic within a specific area or road network through various measures, such as traffic signal optimization, congestion reduction, and enhancing overall transportation systems.

**COMPONENTS**:

* Ultrasonic sensor
* Rasiberry pi
* Resistor
* LED
* Bread board

**Ultrasonic sensor**:

An ultrasonic sensor is a device that uses high-frequency sound waves (ultrasonic waves) to measure distances or detect the presence of objects. It works by emitting a sound wave and then measuring the time it takes for the sound to bounce back after hitting an object. Ultrasonic sensors are commonly used in various applications, including proximity sensing, obstacle detection, and distance measurement.

**Raspberry pi** :

Raspberry Pi is a low-cost, credit card-sized computer designed for educational and hobbyist projects. It's widely used for programming, electronics experimentation, and various applications due to its versatility.

**Resistor**:

A resistor is an electronic component that restricts the flow of electrical current. It is commonly used to control the amount of current or voltage in a circuit and is characterized by its resistance value, measured in ohms (Ω). Resistors are integral in various electronic applications, from voltage division to current limiting and signal conditioning.


**LED**:


An LED (Light Emitting Diode) is a semiconductor device that emits light when an electric current passes through it. LEDs are commonly used for various applications, including lighting, displays, indicators, and as low-energy light sources due to their efficiency and longevity.

**Cloud platform**:

Cloud platforms are used in traffic management projects to centralize data, provide real-time analytics, and enable remote access to traffic information. They offer scalability, reliability, and the ability to process and store large volumes of data from sensors and cameras for improved traffic control and decision-making.

**OUTPUT**:





Simulation link:

[https://wokwi.com/projects/380209624943953921](../Desktop/nm%20iot.html)

Team members:

1. KAVIYA T V 2021504016
2. ANUSNEKHAA L N 2021504503
3. DAINTY CHRISTIANA J C R 2021504509
4. HARITHRA R 2021504520